**** HOw to program EPCS16/M25P16  and boot FPGA from it *****

In Quartus Device\Device and Pin options\Configuration in Configuration scheme: select 'Active Serial (can use Configuration Device)'

In Configuration Device select 'EPCS16'

In Programmer select Mode: 'Active Serial Programming'

In file select 'Penelope.pof'

In device select 'EPCS16'

Check Program/Configure and Verify for both lines

Set Jumpers on FPGA board to Active Serial i.e. Config A and B = 0 

Program!





